**New Requirement: Manual operated hydraulic press**

**Hydraulic Press-1Nos**

Application : Crusher(Organic/food items)

Capacity : 600bar load

Cylinder : Cast iron, Dia 7”

Cylinder surface coat : Food grade

Travel length : 400mm

top plate rigid

bottom plate move upwards, hydraulic assisted manual operating machine required

Reference Machine:

